

Attachment 1 to PAT-1400-25
Pittsburgh Regional Transit Coach Bus and Brake Lining Information

	Year
	Mfg.
	Model
	Coach
Style
	Series Range
	GVWR
	Front Axle
	Rear Axle
	Center Axle
	Unladen
Weight
	Axle Models
	Front Shoe/Lining ID
	PAAC Stock No.
	Rear Shoe/Lining ID
	PAAC Stock No.

	2014
	Gillig
	G27D102N4
	Low Floor
	6001-6060
	39,600
	14,600
	25,000
	N/A
	28,340
	(1)
	4715 STD
	963060
	4592 Full Bushing
	893032

	2015
	Gillig
	G27B102N4
	Low Floor
	1701-1730
	39,600
	14,600
	25,000
	N/A
	27,560
	(1)
	4715 STD
	963060
	4592 Full Bushing
	893032

	2015
	Gillig
	G27D102N4
	Low Floor
	6101-6060
	39,600
	14,600
	25,000
	N/A
	28,640
	(1)
	4715 STD
	963060
	4592 Full Bushing
	893032

	2016
	Gillig
	G27D102N4
	Low Floor
	6201-6275
	39,600
	14,600
	25,000
	N/A
	28,820
	(1)
	4715 STD
	963060
	4592 Full Bushing
	893032




Axle Models:  	(1)  Front: Arvin-Meritor FH946,  Rear: Arvin-Meritor 71163     
	(2)  Front: MAN V8 65L,  Center: MAN Hong 1100,  Rear: MAN HP-1352-HF



